






TCP Port setting for Mnova Client (UNIST)

1. Go to Start button-Control panel-Window firewall



1. Click “Advanced setting”
2. Click the “Inbounded rule”   
   
3. Click “New rule”  
   
4. Check “Port”  
   
5. Put the Port number “15500” 
6. Put the name “Mnova” and description “15500port” and click the “Finish”
7. You can see the 15500 Port as Mnova in the bounce list 

9. Close the window and restart the Mnova

-End-